LED safety luminaire for illuminating escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.Bar-shaped plastic housing with clear trapezoidal cover for wall or ceiling mounting. Optionally, the luminaire can be installed in the ceiling with a mounting frame.Optimum light distribution and illumination of escape and rescue routes is achieved by using diffuser lenses and powerful LED ERT technology.

Material: Plastic
Color: RAL 9003
Dimensions: 332 mm x 48 mm x 72 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 4,6 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: KEU029

Accessories:
lbl-articleNumber: DSA, cord suspension set 1,5m
lbl-articleNumber: KEE-EB, KE recessed frame with test button self-contained
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KXBE, KX concrete box 01+02

Brand: RP-Technik GmbH
