Emergency sign luminaire in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim synthetic luminaire for universal mounting (wall/ceiling) as well as a wall brackets via the included adapter. With additional downwards light emission. Housing can be opened without the use of tools.  Suitable for continuous mode or stand-by mode. The toolless Change and variable use of the pictograms provide planning security on site. Set of pictograms (left, right, bottom, top) is included in the scope of delivery. 

Material: Plastic
Color: RAL 9003
Dimensions: 78 mm x 390 mm x 220 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 43
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 34m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 300 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: KLU019

Accessories:
lbl-articleNumber: DSA, cord suspension set 1,5m
lbl-articleNumber: BALL2, Ball protection (8W) 450x280x125mm  RAL9010, for KCW, KL, LX, VX, PFW
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB

Brand: RP-Technik GmbH
