General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Square recessed LED panel with all-round frame as general luminaire with emergency lighting function. Universally applicable, e.g. in system ceilings with concealed or visible trunking.
Material: Metal
Dimensions: 620 mm x 620 mm x 10 mm
Diameter:  mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: 0 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 36 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 3600 lm lm

Battery: 

lbl-articleNumber: ROPA4201

Accessories:

Brand: RP-Technik GmbH
