LED recessed and surface-mounted downlight, DOALA series, for ceiling recesses of 65 mm to 205 mm. Housing made from aluminium, white, powder-coated. Diffuser made from PS, opal. Operating unit integrated (can be switched). Three-stage adjustment of colour temperature (3000K, 4000K, 5700K) using DIP switch. Version with CASAMBI Bluetooth control available.

label.zuordnungsspeicher.gruppe.CutoutDimensions:

label.zuordnungsspeicher.gruppe.ColorInformation:

label.zuordnungsspeicher.gruppe.MaterialData:

label.zuordnungsspeicher.gruppe.RatingsCertifications:
label.zuordnungsspeicher.IngressProtection: IP 20

label.zuordnungsspeicher.gruppe.ElectricalConnectionLight:
label.zuordnungsspeicher.ContinuousPower: 17 W
label.zuordnungsspeicher.MaxInputVoltageAC: 220-240V / 50-60Hz V

label.zuordnungsspeicher.gruppe.PowerSupplyGeneral:
label.zuordnungsspeicher.DCSuitable: wert.DCSuitable.Nein

label.zuordnungsspeicher.gruppe.LightData:
label.zuordnungsspeicher.LightSource: wert.LightSource.LED
label.zuordnungsspeicher.LuminousFluxIlluminant: 1650 lm
label.zuordnungsspeicher.Colortemperature: 3000/4000/6000 K
label.zuordnungsspeicher.UGR: 27.5

label.zuordnungsspeicher.gruppe.Temperatures:

label.zuordnungsspeicher.gruppe.Mounting:

label.zuordnungsspeicher.gruppe.Dimensions:
label.zuordnungsspeicher.Height: 15 mm
label.zuordnungsspeicher.Diameter: 235 mm

label.zuordnungsspeicher.gruppe.PackageDimensions:

Brand: RP-Technik GmbH
