LED safety light for integrated ceiling mounting for the illumination of emergency and escape routes, in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   The IL recessed luminaire is equipped with an innovative, extremely time saving integrated ceiling mount mechanism. The luminaire consists of only 2 parts, whereby the ceiling mount body includes terminals as well as the tension relief device. The luminaire itself can be mounted tool free and has zero potential when dismantled.Exceptionally efficient because of it’s modern light technology. Therefore, large mounting distances of > 12m are realizable. The dispersion characteristic is rotationally symmetric round. The design of the IL luminaire convinces through it’s timeless elegance.

lbl-monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
lbl-material: Plastic
lbl-color: RAL 9003
maße:  mm x  mm x 84 mm
~lbl-lv-diameter: 122 mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
allowed-temperature-ds: -5 °C To 40 °C celsius
allowed-temperature-bs: -5 °C To 40 °C celsius
lbl-pictogram: Nein

~lbl-lv-LeistungDauerbetrieb: 2,3 W W
~lbl-lv-LeistungBereitschaftsbetrieb: 0,4 W W
~lbl-lv-LichtstromNotbetrieb: 250 lm lm

~lbl-lv-EingangsspannungAC: 230 V V
~lbl-lv-Anschlussquerschnitt: 2.5 mm² mm

lbl-batterie: LFP3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

lbl-articleNumber: ILEL421WL

lbl-zubehoer:
lbl-articleNumber: BALLPLX-ILE, Ball protection  190x190x62mm incl. fastening Plexiglas clear for ILE
lbl-articleNumber: LSYS-B4, 4x Beam lens for lights with a lens system, for example for lighting first aid or fire alarm
lbl-articleNumber: LSYS-F4, 4x corridor lenses for luminaires with lens system
lbl-articleNumber: LSYS-R4, 4x  round lenses for luminaires with lens system
lbl-articleNumber: LSYS-S4, 4x Spotlens for luminares with lens system. Suitable for ceilings up to 12m

~lbl-lv-manufacturer-addendum
