LED safety light for integrated ceiling mounting for the illumination of emergency and escape routes, in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   The IL recessed luminaire is equipped with an innovative, extremely time saving integrated ceiling mount mechanism. The luminaire consists of only 2 parts, whereby the ceiling mount body includes terminals as well as the tension relief device. The luminaire itself can be mounted tool free and has zero potential when dismantled.Exceptionally efficient because of it’s modern light technology. Therefore, large mounting distances of > 12m are realizable. The dispersion characteristic is rotationally symmetric round. The design of the IL luminaire convinces through it’s timeless elegance.

lbl-material: Plastic
lbl-color: RAL 9003
maße:  mm x  mm x 84 mm
~lbl-lv-diameter: 122 mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 3
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
allowed-temperature-ds: -5 °C To 40 °C celsius
allowed-temperature-bs: -5 °C To 40 °C celsius
lbl-pictogram: Nein

~lbl-lv-LeistungDauerbetrieb: 2,8 W W
~lbl-lv-LeistungBereitschaftsbetrieb: 0,4 W W
~lbl-lv-LichtstromNotbetrieb: 360 lm lm

~lbl-lv-EingangsspannungAC: 24 V V
~lbl-lv-Anschlussquerschnitt: 2.5 mm² mm

lbl-batterie: 

lbl-articleNumber: ILEL529CC

lbl-zubehoer:
lbl-articleNumber: BALLPLX-ILE, Ball protection  190x190x62mm incl. fastening Plexiglas clear for ILE
lbl-articleNumber: ILE-OEF-PC, IL recessed opener plastic

~lbl-lv-manufacturer-addendum
