Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Mounting method: Wandeinbau
Protection class: 1
Viewing distance: 20m m
Pictogram: Set

Article number: UEMR411WL

Accessories:

Brand: RP-Technik GmbH
