
Material: Plastic
Color: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm
Diameter:  mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 9 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 780 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: PMW039

Accessories:
Article number: LSYS-B4, 4x Beam lens for lights with a lens system, for example for lighting first aid or fire alarm
Article number: LSYS-F4, 4x corridor lenses for luminaires with lens system
Article number: LSYS-H4, 4x h-lenses for luminaires with lens system
Article number: LSYS-R4, 4x  round lenses for luminaires with lens system
Article number: LSYS-S4, 4x Spotlens for luminares with lens system. Suitable for ceilings up to 12m

Brand: RP-Technik GmbH
