Emergency sign / safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.Cuboid shaped synthetic housing, minimalistic design, reduced on the important aspects.Module-based construction, universal mounting (wall/ceiling surface mount/integrated ceiling mount*/brackets*).  For the use as a safety light without applying the pictograms. Due to the modular system, the safety light can be converted to an escape sign luminaire at any time, without dismantling or the use of tools. It is also possible to mount 3 different sized panels to realize recognition ranges of 14 – 30m. Reliable planning due to a toolfree and variable, on-site use of the pictograms. Pluggable set of pictograms (left, right, bottom, neutral) is included in the scope of delivery (KBK, KBM, KBG). The use diffusion lenses and the efficient LED ERT technology, leads to ideal light distribution and illumination of emergency escape routes. This way, greatly increased mounting distances are made possible. * with an additional adapter

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Plastic
Color: RAL 9003
Dimensions: 326 mm x 50 mm x 50 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 64
lbl-impactResistanceRate: IK 5
Allowed temperature DS: -5 °C to 35 °C °C
Allowed temperature BS: -5 °C to 35 °C °C
Viewing distance: 14m,22m,30m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 460 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

lbl-articleNumber: KBU421WL

Accessories:
lbl-articleNumber: KBK, KB disc VD 14m incl. pictoset
lbl-articleNumber: KBM, KB disc VD 22m incl. pictoset
lbl-articleNumber: KBG, KB disc VD 30m incl. pictoset
lbl-articleNumber: AWX001, Wall bracket, white convenient for RX, KB, KX, KW, LX, GX, KE
lbl-articleNumber: KBE, KB recessed frame - ABS white  exkl. test button
lbl-articleNumber: BALLPLX-KBE, Ball protection  465x181x31mm incl. fastening Plexiglas clear for KBU recessed
lbl-articleNumber: BALLPLX-KBS, Ball protection 410x322x77mm incl. fastening Plexiglas clear for KB incl. edge
lbl-articleNumber: BALLPLX-KBU, Ball protection 420x150x77mm outside Plexiglas clear, for KB witout edge
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KBBE
lbl-articleNumber: DSA, cord suspension set 1,5m
lbl-articleNumber: LSYS-B4, 4x Beam lens for lights with a lens system, for example for lighting first aid or fire alarm
lbl-articleNumber: LSYS-F4, 4x corridor lenses for luminaires with lens system
lbl-articleNumber: LSYS-H4, 4x h-lenses for luminaires with lens system
lbl-articleNumber: LSYS-R4, 4x  round lenses for luminaires with lens system
lbl-articleNumber: LSYS-S4, 4x Spotlens for luminares with lens system. Suitable for ceilings up to 12m

Brand: RP-Technik GmbH
