Four-sided LED escape sign luminaire for ceiling mounting according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838. Cube plastic luminaire with frameless bonnet and easy-to-mount bayonet catch. Due to the stable construction, the luminaire can also be suspended by chain or rope. Suitable for continuous or stand-by operation. Planning reliability thanks to logically printed pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom) as standard.
lbl-monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
lbl-material: Plastic
lbl-color: RAL 9003
maße: 500 mm x 522 mm x 280 mm
~lbl-lv-diameter:  mm

lbl-mountingMethod: Decke
lbl-protectionClass: 2
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK ≥ 3
~lbl-lv-erkennungsweite: 50m m
lbl-pictogram: Set

lbl-articleNumber: WHGD413SC

lbl-zubehoer:
lbl-articleNumber: LFP3233-SET-2AKKU

~lbl-lv-manufacturer-addendum
