
Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system

Power maintained mode: 3,2 W W
Power non-maintained mode: 1 W W
Luminous Flux Emergency Operation: 220 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: KSU019ML-SW

Accessories:

Brand: RP-Technik GmbH
