Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Plastic
Color: RAL 9003
Dimensions: 212 mm x 31 mm x 141 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK 5
Allowed temperature DS: -30 °C to 40 °C °C
Allowed temperature BS: -30 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 2,7 W W
Power non-maintained mode: 0,9 W W

Battery: 

lbl-articleNumber: KFMU009ML

Accessories:

Brand: RP-Technik GmbH
