Emergency sign luminaire in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Innovative synthetic edge luminaire for universal mounting (wall/ceiling surface mount/integrated ceiling mount*/brackets*). Tapered housing for an appealing appearance. Suitable for continuous mode or stand-by mode. Reliable planning due to a toolless and variable, on-site use of the pictograms. Pluggable set of pictograms (left, right, down, top) is included in the scope of delivery. 

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Plastic
Color: RAL 9003
Dimensions: 48 mm x 332 mm x 242 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 35 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Set

Power maintained mode: 4,3 W W
Power non-maintained mode: 0,7 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3216-SET-2AKKU

lbl-articleNumber: KXU413WL

Accessories:
lbl-articleNumber: KXE-EB, KX - recessed frame SB incl. test button
lbl-articleNumber: AWX001, Wall bracket, white convenient for RX, KB, KX, KW, LX, GX, KE
lbl-articleNumber: DSA, cord suspension set 1,5m
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KXBE, KX concrete box 01+02

Brand: RP-Technik GmbH
