Emergency sign luminaire in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim synthetic luminaire for universal mounting wall/ceiling as well as wall brackets via the included adapter. With additional downwards light emission. Housing can be opened without the use of tools.  Suitable for continuous mode or stand-by mode. Reliable planning due to a toolfree and variable, on-site use of the pictograms. Set of pictograms (left, right, bottom, top) is included in the scope of delivery. 

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Plastic
Color: RAL 9003
Dimensions: 70 mm x 260 mm x 155 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 43
lbl-impactResistanceRate: IK 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 3,5 W W
Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

lbl-articleNumber: KDU411WL

Accessories:
lbl-articleNumber: DSA, cord suspension set 1,5m
lbl-articleNumber: BALL1, Ball protection (6W) 320x220x120mm  RAL9010, for KD, KM, KS, LM, SD, VM
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: BALLPLX-KD, Ball protection  380x280x100mm incl. fastening Plexiglas clear for KDU wall

Brand: RP-Technik GmbH
