Surveillance: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Matériau: Matière plastique
Couleur: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm
Diamètre:  mm

lbl-mountingMethod: Wand
lbl-protectionClass: 2
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK 6
Température permise en mode contenu: -15 °C à 40 °C °C
Température permise en mode veille: -15 °C à 40 °C °C
Distance de reconnaissance: 20m m
Pictogramme: Set

lbl-articleNumber: PMW403WL-TT

Accessoires:

Marque: RP-Technik GmbH
