
Material: Plast
Color: RAL 9003
Dimensions: 326 mm x 50 mm x 50 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 64
lbl-impactResistanceRate: IK 5
Allowed temperature DS: -30 °C to 35 °C °C
Allowed temperature BS: -30 °C to 35 °C °C
Viewing distance: 14m,22m,30m m
Pictogram: Einzeln n.A.

Power maintained mode: 4,6 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: KBU029

Accessories:
lbl-articleNumber: KBK, 
lbl-articleNumber: KBM, 
lbl-articleNumber: KBG, 
lbl-articleNumber: AWX001, 
lbl-articleNumber: KBE, 
lbl-articleNumber: BALLPLX-KBE, 
lbl-articleNumber: BALLPLX-KBS, 
lbl-articleNumber: BALLPLX-KBU, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KBBE
lbl-articleNumber: DSA, 

Brand: RP-Technik GmbH
