
Material: Metall
Color: RAL 9003
Dimensions: 65 mm x 280 mm x 160 mm
Diameter:  mm

lbl-mountingMethod: Wandeinbau
lbl-protectionClass: 1
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 5,2 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 300 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: U6E019ML

Accessories:
lbl-articleNumber: U6BE, 

Brand: RP-Technik GmbH
