
Material: Metall
Color: RAL 9003
Dimensions: 65 mm x 375 mm x 200 mm
Diameter:  mm

lbl-mountingMethod: Wandeinbau
lbl-protectionClass: 1
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 34m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 300 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: U8E019

Accessories:
lbl-articleNumber: U8BE, 

Brand: RP-Technik GmbH
