
Material: Plast
Color: RAL 9003
Dimensions: 48 mm x 332 mm x 242 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 40
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 300 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: KXU019

Accessories:
lbl-articleNumber: KXE-EB, 
lbl-articleNumber: AWX001, 
lbl-articleNumber: DSA, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KXBE, 

Brand: RP-Technik GmbH
