
Material: Pressstøping av sink
Color: RAL 9003
Dimensions: 166 mm x 21 mm x 106 mm
Diameter:  mm

lbl-mountingMethod: Wandeinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK 7
Allowed temperature DS: -35 °C to 40 °C °C
Allowed temperature BS: -35 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 4,3 W W
Power non-maintained mode: 0,7 W W
Luminous Flux Emergency Operation: 420 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: WEF029ML

Accessories:

Brand: RP-Technik GmbH
