
Material: Pressstøping av sink
Color: RAL 7016
Dimensions: 79 mm x 241 mm x 159 mm
Diameter:  mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 3,5 W W
Power non-maintained mode: 1,1 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: AMCP009ML-AZ

Accessories:
lbl-articleNumber: AM-XBE, 
lbl-articleNumber: AM-X-PKG

Brand: RP-Technik GmbH
