
Material: Pressstøping av sink
Color: Edelstahl
Dimensions: 80 mm x 312 mm x 181 mm
Diameter:  mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Set

Power maintained mode: 3,3 W W
Power non-maintained mode: 0 W W

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: AXCC009-E

Accessories:
lbl-articleNumber: AM-XBE, 

Brand: RP-Technik GmbH
