
Material: Støpt aluminium,Glass
Dimensions: 1360 mm x 157 mm x 197 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 1
lbl-protectionRating: IP 66
lbl-impactResistanceRate: IK 5
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 45 W W
Luminous Flux Emergency Operation: 4600 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: XPXU019

Accessories:
lbl-articleNumber: X-KO001, 
lbl-articleNumber: X-MB001, 
lbl-articleNumber: X-KE001, 
lbl-articleNumber: X4N, 

Brand: RP-Technik GmbH
