
Material: Pressstøping av sink
Color: RAL 9003
Dimensions:  mm x  mm x 106 mm
Diameter: 363 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 1
lbl-protectionRating: IP 54
lbl-impactResistanceRate: IK 10
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 17 W W
Luminous Flux Emergency Operation: 1600 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: QCW009

Accessories:

Brand: RP-Technik GmbH
