
Material: Plast
Color: RAL 9003
Dimensions: 86 mm x 390 mm x 99 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK 6
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 4,6 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: KWIW029

Accessories:
lbl-articleNumber: BKW, 

Brand: RP-Technik GmbH
