
lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: 0 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 33 W W
Power non-maintained mode: 2 W W
Luminous Flux Emergency Operation: 600 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: ROPA4201SC-WW

Accessories:

Brand: RP-Technik GmbH
