
Material: Plast
Color: RAL 9003
Dimensions:  mm x  mm x 84 mm
Diameter: 122 mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 2,3 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 250 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: ILEL423WB

Accessories:
lbl-articleNumber: BALLPLX-ILE, 
lbl-articleNumber: LSYS-B4, 
lbl-articleNumber: LSYS-F4, 
lbl-articleNumber: LSYS-R4, 
lbl-articleNumber: LSYS-S4, 

Brand: RP-Technik GmbH
