
Material: Pressstøping av sink
Color: RAL 9003
Dimensions: 92 mm x 236 mm x 291 mm
Diameter:  mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 2,5 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 165 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: AMEP509CC

Accessories:
lbl-articleNumber: AM-X-PKG

Brand: RP-Technik GmbH
