
Material: Pressstøping av sink
Color: RAL 9003
Dimensions: 166 mm x 21 mm x 106 mm
Diameter:  mm

lbl-mountingMethod: Wandeinbau
lbl-protectionClass: 3
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK 7
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 3,3 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 420 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: WEF529CC

Accessories:

Brand: RP-Technik GmbH
