
Material: Aluminium
Color: RAL 9003
Dimensions:  mm x  mm x 113 mm
Diameter: 395 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 1
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 28 W W
Power non-maintained mode: 2 W W
Luminous Flux Emergency Operation: 360 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: LFP3245.WRLED

lbl-articleNumber: QAW403SC-SI-BM

Accessories:

Brand: RP-Technik GmbH
