
Material: Plast
Color: RAL 9003
Dimensions: 86 mm x 390 mm x 99 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 460 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: KWIW421WL

Accessories:
lbl-articleNumber: BKW, 
lbl-articleNumber: LSYS-B4, 
lbl-articleNumber: LSYS-F4, 
lbl-articleNumber: LSYS-H4, 
lbl-articleNumber: LSYS-R4, 
lbl-articleNumber: LSYS-S4, 

Brand: RP-Technik GmbH
