
Material: Aluminium
Color: Alu eloxiert
Dimensions:  mm x  mm x 113 mm
Diameter: 395 mm

lbl-mountingMethod: Universal
lbl-protectionClass: 1
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -20 °C to 30 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 27,2 W W
Power non-maintained mode: 1,2 W W
Luminous Flux Emergency Operation: 360 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

lbl-articleNumber: QAW029ML-BM

Accessories:

Brand: RP-Technik GmbH
