
Material: Plast
Color: RAL 9003
Dimensions: 326 mm x 50 mm x 50 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 64
lbl-impactResistanceRate: IK 5
Allowed temperature DS: -5 °C to 35 °C °C
Allowed temperature BS: -5 °C to 35 °C °C
Viewing distance: 14m,22m,30m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 85 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: KBU428WL

Accessories:
lbl-articleNumber: KBK, 
lbl-articleNumber: KBM, 
lbl-articleNumber: KBG, 
lbl-articleNumber: AWX001, 
lbl-articleNumber: KBE, 
lbl-articleNumber: BALLPLX-KBE, 
lbl-articleNumber: BALLPLX-KBS, 
lbl-articleNumber: BALLPLX-KBU, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: KBBE
lbl-articleNumber: DSA, 
lbl-articleNumber: LSYS-B4, 
lbl-articleNumber: LSYS-F4, 
lbl-articleNumber: LSYS-H4, 
lbl-articleNumber: LSYS-R4, 
lbl-articleNumber: LSYS-S4, 

Brand: RP-Technik GmbH
