
Material: Pressstøping av sink
Color: RAL 9003
Dimensions: 58 mm x 262 mm x 188 mm
Diameter:  mm

lbl-mountingMethod: Decke
lbl-protectionClass: 1
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK 8
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3233-SET-2AKKU

lbl-articleNumber: FMDS423WL

Accessories:
lbl-articleNumber: FMDA001, 
lbl-articleNumber: FMDA002, 
lbl-articleNumber: FMDA001-AZ, 
lbl-articleNumber: FMDA002-AZ, 
lbl-articleNumber: FMWA001, 
lbl-articleNumber: FMFH, 

Brand: RP-Technik GmbH
