
Material: Plast
Color: RAL 9005
Dimensions: 34 mm x 250 mm x 174 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 54
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 3,9 W W
Power non-maintained mode: 1,5 W W
Luminous Flux Emergency Operation: 85 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: KSU018WL-SW

Accessories:
lbl-articleNumber: KME-EB, 
lbl-articleNumber: AWKSU, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: KMBE, 
lbl-articleNumber: BALLPLX-KMU, 
lbl-articleNumber: DSA, 
lbl-articleNumber: KSE-MB-WS, 
lbl-articleNumber: KSE-MB-SI, 

Brand: RP-Technik GmbH
