
Material: Pressstøping av sink
Color: RAL 9003
Dimensions: 90 mm x 19 mm x 90 mm
Diameter:  mm

lbl-mountingMethod: Wandeinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 1,9 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 140 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

lbl-articleNumber: WER029

Accessories:

Brand: RP-Technik GmbH
