
Material: Plast
Color: RAL 9003
Dimensions: 78 mm x 390 mm x 220 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 43
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 34m m
Pictogram: Set

Power maintained mode: 7,5 W W
Power non-maintained mode: 3,6 W W
Luminous Flux Emergency Operation: 150 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMH1208P, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: KLU013WLSE

Accessories:
lbl-articleNumber: DSA, 
lbl-articleNumber: BALL2, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB

Brand: RP-Technik GmbH
