
Material: Pressstøping av sink
Color: RAL 7016
Dimensions: 79 mm x 236 mm x 165 mm
Diameter:  mm

lbl-mountingMethod: Deckeneinbau
lbl-protectionClass: 2
lbl-protectionRating: IP 20
lbl-impactResistanceRate: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 3,5 W W
Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: AMCC403WL-AZ

Accessories:
lbl-articleNumber: AM-XBE, 
lbl-articleNumber: LFP3212-LEO, 

Brand: RP-Technik GmbH
