Material: Pressstøping av sink
Color: RAL 7016
Dimensions: 58 mm x 262 mm x 188 mm
Diameter:  mm

lbl-mountingMethod: Wand
lbl-protectionClass: 1
lbl-protectionRating: IP 65
lbl-impactResistanceRate: IK 8
Allowed temperature DS: -15 °C to 40 °C °C
Allowed temperature BS: -15 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

lbl-articleNumber: FMW403SC-TT-AZ

Accessories:
lbl-articleNumber: FMWA001, 
lbl-articleNumber: FMDA001, 
lbl-articleNumber: FMDA002-AZ, 
lbl-articleNumber: FMFH, 
lbl-articleNumber: FMDA001-AZ, 
lbl-articleNumber: FMDA002, 

Brand: RP-Technik GmbH
