
Material: Plast
Color: RAL 9003
Dimensions: 70 mm x 260 mm x 155 mm
Diameter:  mm

lbl-mountingMethod: Universal
lbl-protectionClass: 2
lbl-protectionRating: IP 43
lbl-impactResistanceRate: IK 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 3,5 W W
Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFP3212-LEO, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batteri

lbl-articleNumber: KDU418WL

Accessories:
lbl-articleNumber: DSA, 
lbl-articleNumber: BALL1, 
lbl-articleNumber: 2PW-EB
lbl-articleNumber: 2DW-EB
lbl-articleNumber: BALLPLX-KD, 

Brand: RP-Technik GmbH
